Heater Instructions:
Starting:
- Quick push on the Power button. This enters into the startup mode. The unit glow plug light will illuminate, the fan will begin to spin on low, increasing as the unit warms up. As the unit warms, you will notice the fuel pump clicking sound indicating it is working. The glow plug light will turn off after unit starts to get warm. You will notice some smoke from the muffler until the unit fully heats up. After the unit fully heats up the fan may drop to medium speed. Once at temp the fan will continue to run at low speed.  

Stopping:
- Press power button for 4 seconds, wait till unit powers off. It will take a few minutes as it enters a cool-off and power down mode.
Changing Temp:
-Use the top or bottom arrows to either raise or lower it, the fan still runs all the time, but the speed will change depending on temp. If changing temp is in HZ, press the top 2 buttons simultaneous and it will change to Celcius.
- When unit gets to set temperature it never shuts off, it just runs at low speed.

Timers:
- There are 2 Timers built in.

Priming Fuel Lines:
Press Down arrow and Settings button till you see Ho, change setting to On and this will run the pump for a few minutes to prime, watch line and shutoff when fuel gets to unit. Shutoff by changing Ho setting to off.

NOTES:
- This is a Chinese Diesel Heater 5kw version.
- If the controller fails or is unplugged the unit continues to run, if power is pulled the unit will overheat and possibly damage the controller board in the main unit. Keep a spare controller (eBay), and swap it in if the controller dies.
- To be safe use with a Carbon monoxide/Fire Alarm.